**Go Back N ARQ protocol:-**

**CODE:-**

#include<iostream>

#include <time.h>

#include <cstdlib>

#include<ctime>

#include <unistd.h>

using namespace std;

class timer {

private:

unsigned long begTime;

public:

void start() {

begTime = clock();

}

unsigned long elapsedTime() {

return ((unsigned long) clock() - begTime) / CLOCKS\_PER\_SEC;

}

bool isTimeout(unsigned long seconds) {

return seconds >= elapsedTime();

}

};

int main()

{

int frames[] = {1,2,3,4,5,6,7,8,9,10};

unsigned long seconds = 5;

srand(time(NULL));

timer t;

cout<<"Sender has to send frames : ";

for(int i=0;i<10;i++)

cout<<frames[i]<<" ";

cout<<endl;

int count = 0;

bool delay = false;

cout<<endl<<"Sender\t\t\t\t\tReceiver"<<endl;

do

{

bool timeout = false;

cout<<"Sending Frame : "<<frames[count];

cout.flush();

cout<<"\t\t";

t.start();

if(rand()%2)

{

int to = 24600 + rand()%(64000 - 24600) + 1;

for(int i=0;i<64000;i++)

for(int j=0;j<to;j++) {}

}

if(t.elapsedTime() <= seconds)

{

cout<<"Received Frame : "<<frames[count]<<" ";

if(delay)

{

cout<<"Duplicate";

delay = false;

}

cout<<endl;

count++;

}

else

{

cout<<"---"<<endl;

cout<<"Timeout"<<endl;

timeout = true;

}

t.start();

if(rand()%2 || !timeout)

{

int to = 24600 + rand()%(64000 - 24600) + 1;

for(int i=0;i<64000;i++)

for(int j=0;j<to;j++) {}

if(t.elapsedTime() > seconds )

{

cout<<"Delayed Ack"<<endl;

count--;

delay = true;

}

else if(!timeout)

cout<<"Acknowledgement : "<<frames[count]-1<<endl;

}

}while(count!=10);

return 0;

}

**Output :-**

Enter the number of frames: 10

Enter the Window Size : 3

Sent Frame 1

Sent Frame 2

Sent Frame 3

Acknowledgment for Frame 1

Acknowledgment for Frame 2

Acknowledgment for Frame 3

Sent Frame 4

Sent Frame 5

Sent Frame 6

Frame 4 Not Received

Retransmitting Window

Sent Frame 4

Sent Frame 5

Sent Frame 6

Acknowledgment for Frame 4

Acknowledgment for Frame 5

Acknowledgment for Frame 6

Sent Frame 7

Sent Frame 8

Sent Frame 9

Acknowledgment for Frame 7

Acknowledgment for Frame 8

Acknowledgment for Frame 9

Sent Frame 10

Acknowledgment for Frame 10

Total number of transmissions: 13